

The API of the camera must be configured according to the following configuration

****

Streaming video according to the following configuration



Enter the opening code that has been entered in the ONNA configurator



In the directory we will enter sip:onna@ followed by the IP address of the ONNA touch screen.



Now we will have to link the call to the user created to the button or to the display of the 2N panel. In the case of the touch display, we will introduce the users that we have created as follows. The same is done on the call button.

****